IFC building model
Schema: "IFC4"
Description: "ViewDefinition [DesignTransferView_V1.0]"
Description: "ExchangeRequirement [Architecture]"
Time stamp: "2021-06-25T20:52:39"
Originating system: "Lexocad"
Application: "Lexocad" version "28, 0, 0, 35482" identifier "LX_SUBPRODUCTID: 2800" by Organization "Cadwork Informatik AG, CH - 4051 Basel"

People and organizations
  Person "user" "unknown" of Organization "unknown" description "organization"
  Owner history of Person "user" "unknown" of Organization "unknown" description "organization" | application "Lexocad" version "28, 0, 0, 35482" identifier "LX_SUBPRODUCTID: 2800" by Organization "Cadwork Informatik AG, CH - 4051 Basel" | change ADDED | created 1624647159 (2021-06-25T18:52:39Z) | last modified 1624647159 (2021-06-25T18:52:39Z)

Units
  LENGTHUNIT: METRE
  PLANEANGLEUNIT: RADIAN

Spatial structure
IFCPROJECT
  IFCSITE "Haus am See"
    IFCBUILDING "Gebäude"
      IFCBUILDINGSTOREY "EG" | elevation 0.000000000000000
        contains 12 elements
          1 x IFCSTAIR | type IFCSTAIRTYPE "Treppe" | object type "Treppe" | material: "Beton" | property sets: Pset_StairCommon, lx_global
          2 x IFCSLAB | type IFCSLABTYPE "Decke" | object type "Decke" | FLOOR | material: "Beton" | property sets: Qto_SlabBaseQuantities, Pset_SlabCommon, lx_global, L10.2
          4 x IFCWALL | type IFCWALLTYPE "Wand 2x Typ 2" | STANDARD | material: "Beton" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, lx_global, L10.2, Pset_ManufacturerTypeInformation, ePset_ManufacturerProductInformation
          2 x IFCANNOTATION
          3 x IFCWALL | type IFCWALLTYPE "Wand 2x Typ 2" | STANDARD | material: "Beton" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, lx_global, L10.2
      IFCBUILDINGSTOREY "UG" | elevation -2.700000000000000
        contains 9 elements
          1 x IFCSLAB | type IFCSLABTYPE "Bodenplatte" | object type "Bodenplatte" | FLOOR | material: "Beton" | property sets: Qto_SlabBaseQuantities, Pset_SlabCommon, L10.1, lx_global
          1 x IFCSTAIR | type IFCSTAIRTYPE "Treppe" | object type "Treppe" | material: "Beton" | property sets: Pset_StairCommon, lx_global
          3 x IFCWALL | type IFCWALLTYPE "Wand 2x Typ 2" | STANDARD | material: "Beton" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, lx_global, L10.2
          4 x IFCWALL | type IFCWALLTYPE "Wand 2x Typ 2" | STANDARD | material: "Beton" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, ePset_ManufacturerProductInformation, L10.2, lx_global, Pset_ManufacturerTypeInformation
      IFCBUILDINGSTOREY "OG" | elevation 2.700000000000000
        contains 8 elements
          4 x IFCWALL | type IFCWALLTYPE "Wand 2x Typ 2" | STANDARD | material: "Beton" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, ePset_ManufacturerProductInformation, Pset_ManufacturerTypeInformation, lx_global, L10.2
          3 x IFCWALL | type IFCWALLTYPE "Wand 2x Typ 2" | STANDARD | material: "Beton" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, lx_global, L10.2
          1 x IFCSLAB | type IFCSLABTYPE "Decke" | object type "Decke" | FLOOR | material: "Beton" | property sets: Qto_SlabBaseQuantities, Pset_SlabCommon, lx_global, L10.2
      IFCBUILDINGSTOREY "Dach" | elevation 3.800000000000000
        contains 284 elements
          45 x IFCMEMBER | type IFCMEMBERTYPE "<Missing in L1.csv>: Sparren" | object type "<Missing in L1.csv>: Sparren" | names: "Sparren", "Pfette", "Schwelle" (+1 more) | property sets: Qto_MemberBaseQuantities, Pset_MemberCommon, lx_global
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "<Missing in L1.csv>: Dacheindeckung" | names: "Ziegel" | property sets: lx_global
          232 x IFCBEAM | type IFCBEAMTYPE "<Missing in L1.csv>: Konterlattung" | object type "<Missing in L1.csv>: Konterlattung" | BEAM | names: "Konterlattung", "Dachlattung" | property sets: Qto_BeamBaseQuantities, Pset_BeamCommon, lx_global
          4 x IFCPLATE | type IFCPLATETYPE "<Missing in L1.csv>: Dachfläche aussen" | object type "<Missing in L1.csv>: Dachfläche aussen" | names: "Batten-Board", "Decking" | property sets: lx_global
          1 x IFCCOVERING | type IFCCOVERINGTYPE "<Missing in L1.csv>: Dacheindeckung" | object type "<Missing in L1.csv>: Dacheindeckung" | names: "Firstpfette" | property sets: lx_global

Types
  IFCSTAIRTYPE "Treppe" | element type "LX_USERDEF_COMPONENT" | USERDEFINED | 2 occurrences | material: "Beton"
  IFCSLABTYPE "Decke" | element type "LX_USERDEF_COMPONENT" | USERDEFINED | 3 occurrences | material: "Beton"
  IFCWALLTYPE "Wand 2x Typ 2" | element type "LX_USERDEF_COMPONENT" | USERDEFINED | 12 occurrences | material: "Beton"
  IFCWALLTYPE "Wand 2x Typ 2" | element type "LX_USERDEF_COMPONENT" | USERDEFINED | 9 occurrences | material: "Beton"
  IFCSLABTYPE "Bodenplatte" | element type "LX_USERDEF_COMPONENT" | USERDEFINED | 1 occurrence | material: "Beton"
  IFCMEMBERTYPE "<Missing in L1.csv>: Sparren" | element type "LX_USERDEF_COMPONENT" | USERDEFINED | 45 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "<Missing in L1.csv>: Dacheindeckung" | element type "LX_USERDEF_COMPONENT" | USERDEFINED | 2 occurrences
  IFCBEAMTYPE "<Missing in L1.csv>: Konterlattung" | element type "LX_USERDEF_COMPONENT" | USERDEFINED | 232 occurrences
  IFCPLATETYPE "<Missing in L1.csv>: Dachfläche aussen" | element type "LX_USERDEF_COMPONENT" | USERDEFINED | 4 occurrences
  IFCCOVERINGTYPE "<Missing in L1.csv>: Dacheindeckung" | element type "LX_USERDEF_COMPONENT" | USERDEFINED | 1 occurrence

Property sets
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    BuildableArea = 0.000000000000000 (IFCAREAMEASURE)
    Reference = "" (IFCIDENTIFIER)
    TotalArea = 0.000000000000000 (IFCAREAMEASURE)
  Pset_StairCommon | properties | on 2 objects (2 IFCSTAIR)
    FireExit = FALSE (IFCBOOLEAN)
    FireRating = "" (IFCLABEL)
    HandicapAccessible = FALSE (IFCBOOLEAN)
    HasNonSkidSurface = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    NosingLength = 0.000000000000000 (IFCLENGTHMEASURE) [METRE]
    NumberOfRiser = 0 (IFCCOUNTMEASURE)
    NumberOfTreads = 0 (IFCCOUNTMEASURE)
    Reference = "" (IFCIDENTIFIER)
    Status in {"UNSET"} (IFCLABEL)
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 0.200000000000000 [METRE]
    GrossArea = 175.000000000000000
    NetArea = 175.000000000000000
    NetVolume = 34.232000000000006
    Perimeter = 53.000000000000000 [METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 0.200000000000000 [METRE]
    GrossArea = 0.720000000000009
    NetArea = 0.720000000000009
    NetVolume = 0.144000000000002
    Perimeter = 3.400000000000020 [METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 0.200000000000000 [METRE]
    GrossArea = 175.000000000000000
    NetArea = 175.000000000000000
    NetVolume = 35.000000000000028
    Perimeter = 53.000000000000000 [METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 0.200000000000000 [METRE]
    GrossArea = 175.000000000000000
    NetArea = 175.000000000000000
    NetVolume = 34.078399963378942
    Perimeter = 53.000000000000000 [METRE]
  Pset_SlabCommon | properties | on 3 objects (3 IFCSLAB)
    AcousticRating = "" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Compartmentation = FALSE (IFCBOOLEAN)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0.000000000000000 (IFCPLANEANGLEMEASURE) [RADIAN]
    Reference = "" (IFCIDENTIFIER)
    Status in {"UNSET"} (IFCLABEL)
    SurfaceSpreadOfFlame = "" (IFCLABEL)
    ThermalTransmittance = 0.000000000000000 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    AcousticRating = "" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Compartmentation = FALSE (IFCBOOLEAN)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0.000000000000000 (IFCPLANEANGLEMEASURE) [RADIAN]
    Reference = "" (IFCIDENTIFIER)
    Status in {"UNSET"} (IFCLABEL)
    SurfaceSpreadOfFlame = "" (IFCLABEL)
    ThermalTransmittance = 0.000000000000000 (IFCTHERMALTRANSMITTANCEMEASURE)
  Qto_WallBaseQuantities | quantities | on 2 objects (2 IFCWALL)
    GrossFootprintArea = 2.404321289062500
    Height = 2.500000000000000 [METRE]
    NetFootprintArea = 2.404321289062500
    NetVolume = 5.236803222656251
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 2.420000000014424
    Height = 2.500000000000000 [METRE]
    NetFootprintArea = 2.420000000014424
    NetVolume = 5.650000000036059
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 1.178453540802003
    Height = 2.500000000000000 [METRE]
    NetFootprintArea = 1.178453540802003
    NetVolume = 2.559133852004861
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 1.501546669006348
    Height = 2.500000000000000 [METRE]
    NetFootprintArea = 1.501546669006348
    NetVolume = 3.366866672515678
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 2.799999999986662
    Height = 2.500000000000000 [METRE]
    NetFootprintArea = 2.799999999986662
    NetVolume = 6.412999999966688
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 2.419999999954322
    Height = 2.500000000000000 [METRE]
    NetFootprintArea = 2.419999999954322
    NetVolume = 4.989999999885804
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 2.799999999915519
    Height = 2.500000000000000 [METRE]
    NetFootprintArea = 2.799999999915519
    NetVolume = 6.599999999788821
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 1.501546630900994
    Height = 2.500000000000000 [METRE]
    NetFootprintArea = 1.501546630900994
    NetVolume = 3.366866577252508
  Qto_WallBaseQuantities: 12 more contents on 12 objects not shown
  Pset_WallCommon | properties | on 12 objects (12 IFCWALL)
    AcousticRating = "" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Compartmentation = FALSE (IFCBOOLEAN)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
    Status in {"UNSET"} (IFCLABEL)
    SurfaceSpreadOfFlame = "" (IFCLABEL)
    ThermalTransmittance = 0.000000000000000 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 9 objects (9 IFCWALL)
    AcousticRating = "" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Compartmentation = FALSE (IFCBOOLEAN)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
    Status in {"UNSET"} (IFCLABEL)
    SurfaceSpreadOfFlame = "" (IFCLABEL)
    ThermalTransmittance = 0.000000000000000 (IFCTHERMALTRANSMITTANCEMEASURE)
  Qto_MemberBaseQuantities | quantities | on 7 objects (7 IFCMEMBER)
    NetVolume = 0.094574069149559
    OuterSurfaceArea = 3.962368789430113
  Qto_MemberBaseQuantities | quantities | on 2 objects (2 IFCMEMBER)
    NetVolume = 0.094574069149626
    OuterSurfaceArea = 3.962368789431210
  Qto_MemberBaseQuantities | quantities | on 2 objects (2 IFCMEMBER)
    NetVolume = 0.094574069149559
    OuterSurfaceArea = 3.962368789430078
  Qto_MemberBaseQuantities | quantities | on 2 objects (2 IFCMEMBER)
    NetVolume = 0.094574069147812
    OuterSurfaceArea = 3.962368789400549
  Qto_MemberBaseQuantities | quantities | on 2 objects (2 IFCMEMBER)
    NetVolume = 0.094574069146065
    OuterSurfaceArea = 3.962368789371026
  Qto_MemberBaseQuantities | quantities | on 2 objects (2 IFCMEMBER)
    NetVolume = 0.094574069149559
    OuterSurfaceArea = 3.962368789430109
  Qto_MemberBaseQuantities | quantities | on 2 objects (2 IFCMEMBER)
    NetVolume = 0.291999999999998
    OuterSurfaceArea = 8.799999999999965
  Qto_MemberBaseQuantities | quantities | on 2 objects (2 IFCMEMBER)
    NetVolume = 0.094574069147812
    OuterSurfaceArea = 3.962368789400548
  Qto_MemberBaseQuantities: 23 more contents on 24 objects not shown
  Pset_MemberCommon | properties | on 45 objects (45 IFCMEMBER)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
    Roll = 0.000000000000000 (IFCPLANEANGLEMEASURE) [RADIAN]
    Slope = 0.000000000000000 (IFCPLANEANGLEMEASURE) [RADIAN]
    Status in {"UNSET"} (IFCLABEL)
    ThermalTransmittance = 0.000000000000000 (IFCTHERMALTRANSMITTANCEMEASURE)
  Qto_BeamBaseQuantities | quantities | on 5 objects (5 IFCBEAM)
    NetVolume = 0.011943450000004
    OuterSurfaceArea = 1.418603714262945
  Qto_BeamBaseQuantities | quantities | on 5 objects (5 IFCBEAM)
    NetVolume = 0.011943450000005
    OuterSurfaceArea = 1.418603714262952
  Qto_BeamBaseQuantities | quantities | on 5 objects (5 IFCBEAM)
    NetVolume = 0.017739000000000
    OuterSurfaceArea = 2.104829999999994
  Qto_BeamBaseQuantities | quantities | on 5 objects (5 IFCBEAM)
    NetVolume = 0.017739000000000
    OuterSurfaceArea = 2.104830000000009
  Qto_BeamBaseQuantities | quantities | on 3 objects (3 IFCBEAM)
    NetVolume = 0.011943450000004
    OuterSurfaceArea = 1.418603714262940
  Qto_BeamBaseQuantities | quantities | on 3 objects (3 IFCBEAM)
    NetVolume = 0.017739000000000
    OuterSurfaceArea = 2.104830000000001
  Qto_BeamBaseQuantities | quantities | on 3 objects (3 IFCBEAM)
    NetVolume = 0.017739000000001
    OuterSurfaceArea = 2.104830000000065
  Qto_BeamBaseQuantities | quantities | on 3 objects (3 IFCBEAM)
    NetVolume = 0.017739000000000
    OuterSurfaceArea = 2.104829999999970
  Qto_BeamBaseQuantities: 158 more contents on 200 objects not shown
  Pset_BeamCommon | properties | on 232 objects (232 IFCBEAM)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
    Roll = 0.000000000000000 (IFCPLANEANGLEMEASURE) [RADIAN]
    Slope = 0.000000000000000 (IFCPLANEANGLEMEASURE) [RADIAN]
    Status in {"UNSET"} (IFCLABEL)
    ThermalTransmittance = 0.000000000000000 (IFCTHERMALTRANSMITTANCEMEASURE)
  lx_global | properties | on 335 objects (232 IFCBEAM, 45 IFCMEMBER, 24 IFCOPENINGELEMENT, 21 IFCWALL)
  L10.2 | properties | on 24 objects (21 IFCWALL, 3 IFCSLAB)
  ePset_ManufacturerProductInformation | properties | on 9 objects (9 IFCWALL)
    Betontyp nach NPK = "" (IFCLABEL)
    CEM min. = "" (IFCLABEL)
    Category = "" (IFCLABEL)
    Chloridgehaltsklasse = "" (IFCLABEL)
    Description = "" (IFCLABEL)
    Druckfestigkeitsklasse = "" (IFCLABEL)
    E-Modul = "" (IFCLABEL)
    Expositionsklasse = "" (IFCLABEL)
    Frischbetoneigenschaft = "" (IFCLABEL)
    Gesteinskörnung = "" (IFCLABEL)
    Grösstkorn = "" (IFCLABEL)
    Konsistenzklasse = "" (IFCLABEL)
    Recyclingbeton nach SIA Merkblatt 2030 = "" (IFCLABEL)
    Sorten Nummer = "" (IFCLABEL)
    VKF Hagelschutz-Nr. = "" (IFCLABEL)
    max. W/Zeq = "" (IFCLABEL)
  ePset_ManufacturerProductInformation | properties | on 3 objects (3 IFCWALL)
    Betontyp nach NPK = "NPK B" (IFCLABEL)
    CEM min. = "308 kg/m3" (IFCLABEL)
    Category = "https://ch.buildup.group/category/91c1ed6a-ab21-4a53-a8d8-be9a0c06753e/view" (IFCLABEL)
    Chloridgehaltsklasse = "CI 0.10" (IFCLABEL)
    Description = "" (IFCLABEL)
    Druckfestigkeitsklasse = "C25/30" (IFCLABEL)
    E-Modul = ">28 000 N/mm2" (IFCLABEL)
    Expositionsklasse = "XC3" (IFCLABEL)
    Frischbetoneigenschaft = "Pumpbeton" (IFCLABEL)
    Gesteinskörnung = "RC-C" (IFCLABEL)
    Grösstkorn = "16 mm" (IFCLABEL)
    Konsistenzklasse = "C3" (IFCLABEL)
    Recyclingbeton nach SIA Merkblatt 2030 = "Recyclingbeton aus Betongranulat RC-C" (IFCLABEL)
    Sorten Nummer = "B251C" (IFCLABEL)
    VKF Hagelschutz-Nr. = "" (IFCLABEL)
    max. W/Zeq = "0.60" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 9 objects (9 IFCWALL)
    ArticleNumber = "" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    ModelLabel = "" (IFCLABEL)
    ModelReference = "" (IFCLABEL)
    URL = "" (IFCLABEL)
    URL-CitationTime = "" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 3 objects (3 IFCWALL)
    ArticleNumber = "13750" (IFCLABEL)
    Manufacturer = "Eberhard Bau AG" (IFCLABEL)
    ModelLabel = "Hochbaubeton RC-C" (IFCLABEL)
    ModelReference = "C25/30-C3, 16mm, Pumpbeton" (IFCLABEL)
    URL = "https://ch.buildup.group/prd/eberhard-bau-ag/37" (IFCLABEL)
    URL-CitationTime = "2021-06-25T18:46:07.741Z" (IFCLABEL)
  L10.1 | properties | on 1 object (1 IFCSLAB)