IFC building model
Schema: "IFC4"
Description: "ViewDefinition [DesignTransferView_V1.0]"
Description: "ExchangeRequirement [Architecture]"
Time stamp: "2021-06-25T21:09:56"
Originating system: "Lexocad"
Application: "Lexocad" version "28, 0, 0, 35482" identifier "LX_SUBPRODUCTID: 2800" by Organization "Cadwork Informatik AG, CH - 4051 Basel"

People and organizations
  Person "user" "unknown" of Organization "unknown" description "organization"
  Owner history of Person "user" "unknown" of Organization "unknown" description "organization" | application "Lexocad" version "28, 0, 0, 35482" identifier "LX_SUBPRODUCTID: 2800" by Organization "Cadwork Informatik AG, CH - 4051 Basel" | change ADDED | created 1624648196 (2021-06-25T19:09:56Z) | last modified 1624648196 (2021-06-25T19:09:56Z)

Units
  LENGTHUNIT: METRE
  PLANEANGLEUNIT: RADIAN

Spatial structure
IFCPROJECT
  IFCSITE "Haus am See"
    IFCBUILDING "Gebäude"
      IFCBUILDINGSTOREY "EG" | elevation 0.000000000000000
        contains 12 elements
          2 x IFCSLAB | type IFCSLABTYPE "Decke" | object type "Decke" | FLOOR | material: "Beton" | property sets: Qto_SlabBaseQuantities, Pset_SlabCommon, lx_global, L10.2, Pset_ManufacturerTypeInformation, ePset_ManufacturerProductInformation
          3 x IFCWALL | type IFCWALLTYPE "Wand 2x Typ 2" | STANDARD | material: "Beton" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, lx_global, L10.2
          2 x IFCANNOTATION
          4 x IFCWALL | type IFCWALLTYPE "Wand 2x Typ 2" | STANDARD | material: "Beton" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, L10.2, Pset_ManufacturerTypeInformation, lx_global, ePset_ManufacturerProductInformation
          1 x IFCSTAIR | type IFCSTAIRTYPE "Treppe" | object type "Treppe" | material: "Beton" | property sets: Pset_StairCommon, lx_global, ePset_ManufacturerProductInformation, Pset_ManufacturerTypeInformation
      IFCBUILDINGSTOREY "OG" | elevation 2.700000000000000
        contains 8 elements
          3 x IFCWALL | type IFCWALLTYPE "Wand 2x Typ 2" | STANDARD | material: "Beton" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, lx_global, L10.2
          4 x IFCWALL | type IFCWALLTYPE "Wand 2x Typ 2" | STANDARD | material: "Beton" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, lx_global, ePset_ManufacturerProductInformation, L10.2, Pset_ManufacturerTypeInformation
          1 x IFCSLAB | type IFCSLABTYPE "Decke" | object type "Decke" | FLOOR | material: "Beton" | property sets: Qto_SlabBaseQuantities, Pset_SlabCommon, L10.2, ePset_ManufacturerProductInformation, Pset_ManufacturerTypeInformation, lx_global
      IFCBUILDINGSTOREY "Dach" | elevation 3.800000000000000
        contains 284 elements
          4 x IFCPLATE | type IFCPLATETYPE "<Missing in L1.csv>: Dachfläche aussen" | object type "<Missing in L1.csv>: Dachfläche aussen" | names: "Decking", "Batten-Board" | property sets: ePset_ManufacturerProductInformation, Pset_ManufacturerTypeInformation, lx_global
          232 x IFCBEAM | type IFCBEAMTYPE "<Missing in L1.csv>: Konterlattung" | object type "<Missing in L1.csv>: Konterlattung" | BEAM | names: "Konterlattung", "Dachlattung" | property sets: Qto_BeamBaseQuantities, Pset_BeamCommon, Pset_ManufacturerTypeInformation, lx_global, ePset_ManufacturerProductInformation
          45 x IFCMEMBER | type IFCMEMBERTYPE "<Missing in L1.csv>: Sparren" | object type "<Missing in L1.csv>: Sparren" | names: "Sparren", "Pfette", "Firstpfette" (+2 more) | property sets: Qto_MemberBaseQuantities, Pset_MemberCommon, lx_global, Pset_ManufacturerTypeInformation, ePset_ManufacturerProductInformation
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "<Missing in L1.csv>: Dacheindeckung" | names: "Ziegel" | property sets: lx_global, Pset_ManufacturerTypeInformation, ePset_ManufacturerProductInformation
          1 x IFCCOVERING | type IFCCOVERINGTYPE "<Missing in L1.csv>: Dacheindeckung" | object type "<Missing in L1.csv>: Dacheindeckung" | names: "Firstpfette" | property sets: Pset_ManufacturerTypeInformation, ePset_ManufacturerProductInformation, lx_global
      IFCBUILDINGSTOREY "UG" | elevation -2.700000000000000
        contains 9 elements
          1 x IFCSTAIR | type IFCSTAIRTYPE "Treppe" | object type "Treppe" | material: "Beton" | property sets: Pset_StairCommon, lx_global, ePset_ManufacturerProductInformation, Pset_ManufacturerTypeInformation
          4 x IFCWALL | type IFCWALLTYPE "Wand 2x Typ 2" | STANDARD | material: "Beton" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, lx_global, ePset_ManufacturerProductInformation, L10.2, Pset_ManufacturerTypeInformation
          3 x IFCWALL | type IFCWALLTYPE "Wand 2x Typ 2" | STANDARD | material: "Beton" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, lx_global, L10.2
          1 x IFCSLAB | type IFCSLABTYPE "Bodenplatte" | object type "Bodenplatte" | FLOOR | material: "Beton" | property sets: Qto_SlabBaseQuantities, Pset_SlabCommon, L10.1, ePset_ManufacturerProductInformation, lx_global, Pset_ManufacturerTypeInformation

Types
  IFCSLABTYPE "Decke" | element type "LX_USERDEF_COMPONENT" | USERDEFINED | 3 occurrences | material: "Beton"
  IFCWALLTYPE "Wand 2x Typ 2" | element type "LX_USERDEF_COMPONENT" | USERDEFINED | 9 occurrences | material: "Beton"
  IFCWALLTYPE "Wand 2x Typ 2" | element type "LX_USERDEF_COMPONENT" | USERDEFINED | 12 occurrences | material: "Beton"
  IFCSTAIRTYPE "Treppe" | element type "LX_USERDEF_COMPONENT" | USERDEFINED | 2 occurrences | material: "Beton"
  IFCPLATETYPE "<Missing in L1.csv>: Dachfläche aussen" | element type "LX_USERDEF_COMPONENT" | USERDEFINED | 4 occurrences
  IFCBEAMTYPE "<Missing in L1.csv>: Konterlattung" | element type "LX_USERDEF_COMPONENT" | USERDEFINED | 232 occurrences
  IFCMEMBERTYPE "<Missing in L1.csv>: Sparren" | element type "LX_USERDEF_COMPONENT" | USERDEFINED | 45 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "<Missing in L1.csv>: Dacheindeckung" | element type "LX_USERDEF_COMPONENT" | USERDEFINED | 2 occurrences
  IFCCOVERINGTYPE "<Missing in L1.csv>: Dacheindeckung" | element type "LX_USERDEF_COMPONENT" | USERDEFINED | 1 occurrence
  IFCSLABTYPE "Bodenplatte" | element type "LX_USERDEF_COMPONENT" | USERDEFINED | 1 occurrence | material: "Beton"

Property sets
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    BuildableArea = 0.000000000000000 (IFCAREAMEASURE)
    Reference = "" (IFCIDENTIFIER)
    TotalArea = 0.000000000000000 (IFCAREAMEASURE)
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 0.200000000000000 [METRE]
    GrossArea = 175.000000000000000
    NetArea = 175.000000000000000
    NetVolume = 34.232000000000006
    Perimeter = 53.000000000000000 [METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 0.200000000000000 [METRE]
    GrossArea = 0.720000000000009
    NetArea = 0.720000000000009
    NetVolume = 0.144000000000002
    Perimeter = 3.400000000000020 [METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 0.200000000000000 [METRE]
    GrossArea = 175.000000000000000
    NetArea = 175.000000000000000
    NetVolume = 34.078399963378942
    Perimeter = 53.000000000000000 [METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 0.200000000000000 [METRE]
    GrossArea = 175.000000000000000
    NetArea = 175.000000000000000
    NetVolume = 35.000000000000028
    Perimeter = 53.000000000000000 [METRE]
  Pset_SlabCommon | properties | on 3 objects (3 IFCSLAB)
    AcousticRating = "" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Compartmentation = FALSE (IFCBOOLEAN)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0.000000000000000 (IFCPLANEANGLEMEASURE) [RADIAN]
    Reference = "" (IFCIDENTIFIER)
    Status in {"UNSET"} (IFCLABEL)
    SurfaceSpreadOfFlame = "" (IFCLABEL)
    ThermalTransmittance = 0.000000000000000 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    AcousticRating = "" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Compartmentation = FALSE (IFCBOOLEAN)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0.000000000000000 (IFCPLANEANGLEMEASURE) [RADIAN]
    Reference = "" (IFCIDENTIFIER)
    Status in {"UNSET"} (IFCLABEL)
    SurfaceSpreadOfFlame = "" (IFCLABEL)
    ThermalTransmittance = 0.000000000000000 (IFCTHERMALTRANSMITTANCEMEASURE)
  Qto_WallBaseQuantities | quantities | on 2 objects (2 IFCWALL)
    GrossFootprintArea = 2.404321289062500
    Height = 2.500000000000000 [METRE]
    NetFootprintArea = 2.404321289062500
    NetVolume = 5.236803222656251
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 1.178453540802003
    Height = 2.500000000000000 [METRE]
    NetFootprintArea = 1.178453540802003
    NetVolume = 2.559133852004861
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 2.419999999954322
    Height = 2.500000000000000 [METRE]
    NetFootprintArea = 2.419999999954322
    NetVolume = 4.989999999885804
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 2.420000000014424
    Height = 2.500000000000000 [METRE]
    NetFootprintArea = 2.420000000014424
    NetVolume = 5.650000000036059
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 2.799999999915519
    Height = 2.500000000000000 [METRE]
    NetFootprintArea = 2.799999999915519
    NetVolume = 6.599999999788821
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 2.799999999986662
    Height = 2.500000000000000 [METRE]
    NetFootprintArea = 2.799999999986662
    NetVolume = 6.412999999966688
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 1.501546669006348
    Height = 2.500000000000000 [METRE]
    NetFootprintArea = 1.501546669006348
    NetVolume = 3.366866672515678
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    NetVolume = 6.711348553139134
  Qto_WallBaseQuantities: 12 more contents on 12 objects not shown
  Pset_WallCommon | properties | on 12 objects (12 IFCWALL)
    AcousticRating = "" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Compartmentation = FALSE (IFCBOOLEAN)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
    Status in {"UNSET"} (IFCLABEL)
    SurfaceSpreadOfFlame = "" (IFCLABEL)
    ThermalTransmittance = 0.000000000000000 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 9 objects (9 IFCWALL)
    AcousticRating = "" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Compartmentation = FALSE (IFCBOOLEAN)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
    Status in {"UNSET"} (IFCLABEL)
    SurfaceSpreadOfFlame = "" (IFCLABEL)
    ThermalTransmittance = 0.000000000000000 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_StairCommon | properties | on 2 objects (2 IFCSTAIR)
    FireExit = FALSE (IFCBOOLEAN)
    FireRating = "" (IFCLABEL)
    HandicapAccessible = FALSE (IFCBOOLEAN)
    HasNonSkidSurface = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    NosingLength = 0.000000000000000 (IFCLENGTHMEASURE) [METRE]
    NumberOfRiser = 0 (IFCCOUNTMEASURE)
    NumberOfTreads = 0 (IFCCOUNTMEASURE)
    Reference = "" (IFCIDENTIFIER)
    Status in {"UNSET"} (IFCLABEL)
  Qto_BeamBaseQuantities | quantities | on 5 objects (5 IFCBEAM)
    NetVolume = 0.011943450000005
    OuterSurfaceArea = 1.418603714262952
  Qto_BeamBaseQuantities | quantities | on 4 objects (4 IFCBEAM)
    NetVolume = 0.017739000000000
    OuterSurfaceArea = 2.104829999999999
  Qto_BeamBaseQuantities | quantities | on 3 objects (3 IFCBEAM)
    NetVolume = 0.017739000000000
    OuterSurfaceArea = 2.104829999999994
  Qto_BeamBaseQuantities | quantities | on 3 objects (3 IFCBEAM)
    NetVolume = 0.017739000000000
    OuterSurfaceArea = 2.104830000000022
  Qto_BeamBaseQuantities | quantities | on 3 objects (3 IFCBEAM)
    NetVolume = 0.017739000000000
    OuterSurfaceArea = 2.104829999999970
  Qto_BeamBaseQuantities | quantities | on 3 objects (3 IFCBEAM)
    NetVolume = 0.017739000000000
    OuterSurfaceArea = 2.104830000000014
  Qto_BeamBaseQuantities | quantities | on 3 objects (3 IFCBEAM)
    NetVolume = 0.017739000000001
    OuterSurfaceArea = 2.104830000000065
  Qto_BeamBaseQuantities | quantities | on 3 objects (3 IFCBEAM)
    NetVolume = 0.011943450000005
    OuterSurfaceArea = 1.418603714262945
  Qto_BeamBaseQuantities: 168 more contents on 205 objects not shown
  Pset_BeamCommon | properties | on 232 objects (232 IFCBEAM)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
    Roll = 0.000000000000000 (IFCPLANEANGLEMEASURE) [RADIAN]
    Slope = 0.000000000000000 (IFCPLANEANGLEMEASURE) [RADIAN]
    Status in {"UNSET"} (IFCLABEL)
    ThermalTransmittance = 0.000000000000000 (IFCTHERMALTRANSMITTANCEMEASURE)
  Qto_MemberBaseQuantities | quantities | on 6 objects (6 IFCMEMBER)
    NetVolume = 0.094574069149560
    OuterSurfaceArea = 3.962368789430113
  Qto_MemberBaseQuantities | quantities | on 2 objects (2 IFCMEMBER)
    NetVolume = 0.094574069147813
    OuterSurfaceArea = 3.962368789400533
  Qto_MemberBaseQuantities | quantities | on 2 objects (2 IFCMEMBER)
    NetVolume = 0.094574069146066
    OuterSurfaceArea = 3.962368789371026
  Qto_MemberBaseQuantities | quantities | on 2 objects (2 IFCMEMBER)
    NetVolume = 0.094574069149628
    OuterSurfaceArea = 3.962368789431210
  Qto_MemberBaseQuantities | quantities | on 2 objects (2 IFCMEMBER)
    NetVolume = 0.291999999999998
    OuterSurfaceArea = 8.799999999999965
  Qto_MemberBaseQuantities | quantities | on 2 objects (2 IFCMEMBER)
    NetVolume = 0.094574069149561
    OuterSurfaceArea = 3.962368789430078
  Qto_MemberBaseQuantities | quantities | on 2 objects (2 IFCMEMBER)
    NetVolume = 0.094574069149560
    OuterSurfaceArea = 3.962368789430109
  Qto_MemberBaseQuantities | quantities | on 2 objects (2 IFCMEMBER)
    NetVolume = 0.094574069147813
    OuterSurfaceArea = 3.962368789400549
  Qto_MemberBaseQuantities: 23 more contents on 25 objects not shown
  Pset_MemberCommon | properties | on 45 objects (45 IFCMEMBER)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
    Roll = 0.000000000000000 (IFCPLANEANGLEMEASURE) [RADIAN]
    Slope = 0.000000000000000 (IFCPLANEANGLEMEASURE) [RADIAN]
    Status in {"UNSET"} (IFCLABEL)
    ThermalTransmittance = 0.000000000000000 (IFCTHERMALTRANSMITTANCEMEASURE)
  lx_global | properties | on 335 objects (232 IFCBEAM, 45 IFCMEMBER, 24 IFCOPENINGELEMENT, 21 IFCWALL)
  Pset_ManufacturerTypeInformation | properties | on 277 objects (232 IFCBEAM, 45 IFCMEMBER)
    ArticleNumber = "1255958" (IFCLABEL)
    GlobalTradeItemNumber = "EAN: 9010173329663" (IFCLABEL)
    Manufacturer = "EGGER Holzwerkstoffe" (IFCLABEL)
    ModelLabel = "Dachlatten" (IFCLABEL)
    ModelReference = "" (IFCLABEL)
    URL = "https://ch.buildup.group/prd/egger-holzwerkstoffe-schweiz-gmbh/1255958" (IFCLABEL)
    URL-CitationTime = "2021-06-25T19:05:41.617Z" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 9 objects (9 IFCWALL)
    ArticleNumber = "" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    ModelLabel = "" (IFCLABEL)
    ModelReference = "" (IFCLABEL)
    URL = "" (IFCLABEL)
    URL-CitationTime = "" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 4 objects (4 IFCSLAB)
    ArticleNumber = "14304" (IFCLABEL)
    Manufacturer = "Eberhard Bau AG" (IFCLABEL)
    ModelLabel = "Hochbaubeton" (IFCLABEL)
    ModelReference = "C30/37-F3, 32mm, Monobeton" (IFCLABEL)
    URL = "https://ch.buildup.group/prd/eberhard-bau-ag/55" (IFCLABEL)
    URL-CitationTime = "2021-06-25T19:00:49.847Z" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 4 objects (4 IFCPLATE)
    ArticleNumber = "703129" (IFCLABEL)
    GlobalTradeItemNumber = "EAN: 9008283470948" (IFCLABEL)
    Manufacturer = "EGGER Holzwerkstoffe" (IFCLABEL)
    ModelLabel = "OSB 4 TOP Verlegeplatte" (IFCLABEL)
    ModelReference = "OSB 4 TOP CE EAC PMDI MS&DS" (IFCLABEL)
    URL = "https://ch.buildup.group/prd/egger-holzwerkstoffe-schweiz-gmbh/703129" (IFCLABEL)
    URL-CitationTime = "2021-06-25T19:08:38.631Z" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 3 objects (2 IFCBUILDINGELEMENTPROXY, 1 IFCCOVERING)
    ArticleNumber = "" (IFCLABEL)
    Manufacturer = "PREFA Schweiz Vertriebs AG" (IFCLABEL)
    ModelLabel = "PREFA Dachplatte" (IFCLABEL)
    ModelReference = "ziegelrot" (IFCLABEL)
    URL = "https://ch.buildup.group/prd/prefa-schweiz/b_*a10-b_*1" (IFCLABEL)
    URL-CitationTime = "2021-06-25T19:07:36.993Z" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 3 objects (3 IFCWALL)
    ArticleNumber = "13750" (IFCLABEL)
    Manufacturer = "Eberhard Bau AG" (IFCLABEL)
    ModelLabel = "Hochbaubeton RC-C" (IFCLABEL)
    ModelReference = "C25/30-C3, 16mm, Pumpbeton" (IFCLABEL)
    URL = "https://ch.buildup.group/prd/eberhard-bau-ag/37" (IFCLABEL)
    URL-CitationTime = "2021-06-25T18:46:07.741Z" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 2 objects (2 IFCSTAIR)
    ArticleNumber = "14366" (IFCLABEL)
    Manufacturer = "Eberhard Bau AG" (IFCLABEL)
    ModelLabel = "Selbstverdichtender Beton" (IFCLABEL)
    ModelReference = "C30/37-SF2, 16mm, SCC-Beton" (IFCLABEL)
    URL = "https://ch.buildup.group/prd/eberhard-bau-ag/66" (IFCLABEL)
    URL-CitationTime = "2021-06-25T19:03:35.677Z" (IFCLABEL)
  ePset_ManufacturerProductInformation | properties | on 277 objects (232 IFCBEAM, 45 IFCMEMBER)
    Abmessungen Breite = "50.0 mm" (IFCLABEL)
    Abmessungen Länge = "4000.0 mm" (IFCLABEL)
    Abmessungen Stärke = "30.0 mm" (IFCLABEL)
    Basismengeneinheit = "PCE" (IFCLABEL)
    Biologische Dauerhaftigkeit (Gebrauchsklassen) = "Gebrauchsklasse 4" (IFCLABEL)
    Brandklasse = "D-s2, d0" (IFCLABEL)
    Bruttogewicht = "3.0 kg" (IFCLABEL)
    Category = "https://ch.buildup.group/category/036737fc-a969-4c5e-8a72-0ea5c687b9c2/view" (IFCLABEL)
    Description = "EGGER Schnittholz ist frisch, technisch getrocknet oder gehobelt verfügbar. Es wird visuell und maschinell sortiert, damit die optischen Anforderungen und die Festigkeit gewährleistet werden. Dank strikter externer und interner Kontrollen des Schnittholzes, kann die konstant hohe Qualität der Produkte garantiert werden. EGGER Dachlatten aus Fichtenholz werden technisch getrocknet und anschliessend visuell nach DIN 4074-1 S10 sortiert. Jede Dachlatte ist mit einer CE-Kennzeichnung versehen." (IFCLABEL)
    Emissionen = "Keine Substanzen nach SVHV Liste" (IFCLABEL)
    Feuchtegehalt zulässig = "14-18 %" (IFCLABEL)
    Mengeneinheit Gewicht = "KG" (IFCLABEL)
    Produkttyp = "Dachlatten" (IFCLABEL)
    Rohdichte Mindestwert = "360 kg/m³" (IFCLABEL)
    Toleranz Breite = "±1 mm" (IFCLABEL)
    Toleranz Dicke = "±1 mm" (IFCLABEL)
    Toleranz Länge = "5,00 mm" (IFCLABEL)
    Verpackungseinheit = "PA" (IFCLABEL)
    Verpackungsmenge (ST/Paket) = "490 PCE" (IFCLABEL)
    Volumen des Materials = "6000.0 ccm" (IFCLABEL)
  ePset_ManufacturerProductInformation | properties | on 9 objects (9 IFCWALL)
    Category = "" (IFCLABEL)
    Description = "" (IFCLABEL)
  ePset_ManufacturerProductInformation | properties | on 4 objects (4 IFCSLAB)
    Category = "https://ch.buildup.group/category/91c1ed6a-ab21-4a53-a8d8-be9a0c06753e/view" (IFCLABEL)
  ePset_ManufacturerProductInformation | properties | on 4 objects (4 IFCPLATE)
    Abmessungen Breite = "1250.0 mm" (IFCLABEL)
    Abmessungen Länge = "2500.0 mm" (IFCLABEL)
    Abmessungen Stärke = "18.0 mm" (IFCLABEL)
    Basismengeneinheit = "PCE" (IFCLABEL)
    Biegefestigkeit = "31,00 MPa, 18,00 MPa" (IFCLABEL)
    Biologische Dauerhaftigkeit (Gebrauchsklassen) = "GK 1 & 2" (IFCLABEL)
    Brandklasse = "D-s2, d0" (IFCLABEL)
    Bruttogewicht = "34.875 kg" (IFCLABEL)
    Category = "https://ch.buildup.group/category/88b4223e-efb8-4794-90af-ed13474509a9/view" (IFCLABEL)
    Description = "Unsere Egger OSB 4 TOP Verlegeplatte mit Nut- und Federprofil hat viele Eigenschaften, die sogar über den OSB 4 Standard der EN 300 hinausgehen. Mit den ausgezeichneten Festigkeits- und Steifigkeitseigenschaften können auch noch Anwendungen wirtschaftlich realisiert werden, bei denen sonst deutlich teurere Holzwerkstoffplatten oder Massivholz erforderlich sind. Vorteile der OSB 4 TOP Verlegeplatte in der Anwendung - Aufgrund des stabilen und passgenauen Nut- und Federprofils lassen sich die OSB 4 TOP Verlegeplatten schnell und einfach verlegen. - Aufgrund der hohen Biegefestigkeit und Steifigkeit sind unsere OSB 4 TOP immer eine sichere Option zur Herstellung dauerhafter, tragender Dachschalungen und Unterböden auch bei großen Stützweiten. - Für die OSB 4 TOP stellen wir mit der CE-Leistungserklärung (DOP) die geprüften Rechenwerte für den statischen Nachweis sogar für eine Plattendicke von 30 mm zur Verfügung. - Im Unterschied zu OSB 3 besitzt unsere OSB 4 TOP eine geringere Dickenquellung bei Feuchteaufnahme und eine verbesserte Dimensionsstabilität. Dies führt zu mehr Sicherheit beim Transport, während der Bauzeit und im Bauwerk. - Die OSB 4 TOP Verlegeplatten sind aufgrund ihrer hohen Steifigkeit auch bestens für die schwimmende Verlegung geeignet. - Egger OSB 4 TOP Verlegeplatten werden im Dickenbereich von 12 bis 25 mm mit einer garantierten charakteristischen Rohdichte von mehr als 620 kg/m3 produziert. Damit weisen sie eine reduzierte Abbrandrate und Vorteile beim Brandschutznachweis auf." (IFCLABEL)
    Durchstoßfestigkeit (hard body impact) = "No Performance Determined" (IFCLABEL)
    Elastizitätsmodul = "5200 MPa, 2300 MPa" (IFCLABEL)
    Emissionen = "Keine Substanzen nach SVHV Liste" (IFCLABEL)
    Festigkeit Biegung Plattenbeanspruchung ( fm) = "25,00 MPa, 15,00 MPa" (IFCLABEL)
    Festigkeit Biegung Scheibenbeanspruchung (fm) = "22,00 MPa, 17,00 MPa" (IFCLABEL)
    Festigkeit Druck (fc) = "19,00 MPa, 16,00 MPa" (IFCLABEL)
    Festigkeit Druck ┴ zur Plattenebene fc,90 = "10,00 MPa" (IFCLABEL)
    Festigkeit Schub in Plattenebene / Plattenbeanspruchung (fr) = "1,60 MPa" (IFCLABEL)
    Festigkeit Schub ┴ Plattenebene / Scheibenbeanspruchung (fv) = "9,00 MPa" (IFCLABEL)
    Festigkeit Zug (ft) = "12,00 MPa, 10,00 MPa" (IFCLABEL)
    Feuchtegehalt zulässig = "5-12 %" (IFCLABEL)
    Flächenmasse mA = "11,16 kg/m³" (IFCLABEL)
    Formaldehydemission = "<0,03 ppm" (IFCLABEL)
    Formaldehydgehalt JAS Dessicato = "<0,3 mg/L" (IFCLABEL)
    Gebrauchsklasse = "UC2" (IFCLABEL)
    Gehalt an PCP = "<3,0 ppm" (IFCLABEL)
    JAS - Formaldehydklasse = "F****" (IFCLABEL)
    Lochleibungsfestigkeit = "EN 1995-1-1,chp.8 MPa, EN 1995-1-1,chp.8" (IFCLABEL)
    Luftdurchlässigkeit bei Druckdifferenz 50 Pa = "0,12" (IFCLABEL)
    Mechanische Dauerhaftigkeit kdef (NKL 1) = "1,50" (IFCLABEL)
    Mechanische Dauerhaftigkeit kdef (NKL 2) = "2,25" (IFCLABEL)
    Mechanische Dauerhaftigkeit kmod kurz (NKL 1) = "0,90" (IFCLABEL)
    Mechanische Dauerhaftigkeit kmod kurz (NKL 2) = "0,70" (IFCLABEL)
    Mechanische Dauerhaftigkeit kmod lang (NKL 1) = "0,50" (IFCLABEL)
    Mechanische Dauerhaftigkeit kmod lang (NKL 2) = "0,40" (IFCLABEL)
    Mechanische Dauerhaftigkeit kmod mittel (NKL 1) = "0,70" (IFCLABEL)
    Mechanische Dauerhaftigkeit kmod mittel (NKL 2) = "0,55" (IFCLABEL)
    Mechanische Dauerhaftigkeit kmod sehr kurz (NKL 1) = "1,10" (IFCLABEL)
    Mechanische Dauerhaftigkeit kmod sehr kurz (NKL 2) = "0,90" (IFCLABEL)
    Mechanische Dauerhaftigkeit kmod ständig (NKL 1) = "0,40" (IFCLABEL)
    Mechanische Dauerhaftigkeit kmod ständig (NKL 2) = "0,30" (IFCLABEL)
    Mengeneinheit Gewicht = "KG" (IFCLABEL)
    Nutzungsklasse = "SC2" (IFCLABEL)
    PS 2 - Leistungsbewertung Tragender Fußboden = "24 oc 1F24" (IFCLABEL)
    PS 2 Verleimungsklasse = "Exposure 1" (IFCLABEL)
    Performance Boden Plattendicke = "≥18 mm" (IFCLABEL)
    Performance Boden Stützweite = "≤625 mm" (IFCLABEL)
    Performance Dach Plattendicke = "≥18 mm" (IFCLABEL)
    Performance Dach Stützweite = "≤833 mm" (IFCLABEL)
    Performance Wand Plattendicke = "≥9 mm" (IFCLABEL)
    Performance Wand Punktlast/weichem Stoss = "pass" (IFCLABEL)
    Produkttyp = "OSB 4 TOP Verlegeplatte" (IFCLABEL)
    Profil = "T&G" (IFCLABEL)
    Quellung = "10,00 %" (IFCLABEL)
    Querzugfestigkeit - Option 2 = "0,13 MPa" (IFCLABEL)
    Querzugfestigkeit trocken = "0,50 MPa" (IFCLABEL)
    Rohdichte Mindestwert = "620 kg/m³" (IFCLABEL)
    Rohdichte SAP ZSD2 = "620 kg/m³" (IFCLABEL)
    Schallabsorptionskoeffizient = "0,10 Hz, 0,25 Hz" (IFCLABEL)
    Schliff = "ungeschliffen" (IFCLABEL)
    Steifigkeit Biegung Plattenbeanspruchung (Em) = "7000 MPa, 3000 MPa, 3000 MPa" (IFCLABEL)
    Steifigkeit Biegung Scheibenbeanspruchung (Em) = "4200 MPa" (IFCLABEL)
    Steifigkeit Druck (Ec) = "4300 MPa, 3200 MPa" (IFCLABEL)
    Steifigkeit Schub in Plattenebene (Gr) = "160 MPa" (IFCLABEL)
    Steifigkeit Schub ┴ Plattenebene (Gv) = "1500 MPa" (IFCLABEL)
    Steifigkeit Zug (Et) = "4300 MPa, 3200 MPa" (IFCLABEL)
    Techn. Klasse = "OSB/4" (IFCLABEL)
    Toleranz Breite = "±3 mm" (IFCLABEL)
    Toleranz Dicke = "±0,5 mm" (IFCLABEL)
    Toleranz Länge = "±3 mm" (IFCLABEL)
    VOC-Emission = "<1000 µg/m³" (IFCLABEL)
    Verpackungseinheit = "PA" (IFCLABEL)
    Verpackungsmenge (ST/Paket) = "56 PCE" (IFCLABEL)
    Volumen des Materials = "56250.0 ccm" (IFCLABEL)
    Wandscheibensteifigkeit = "EN 1995-1-1" (IFCLABEL)
    Wasserdampfdurchlässigkeit - µ dry = "200,00" (IFCLABEL)
    Wasserdampfdurchlässigkeit - µ wet = "200,00" (IFCLABEL)
    Wärmeleitfähigkeit = "0,13 W/mK" (IFCLABEL)
  ePset_ManufacturerProductInformation | properties | on 3 objects (2 IFCBUILDINGELEMENTPROXY, 1 IFCCOVERING)
    Category = "https://ch.buildup.group/category/41d25de0-580e-4f94-a479-54300fe8cbf7/view" (IFCLABEL)
    Description = "PREFA Dachplatten zählen mit nur 2,3 kg/m² zu den leichtesten aber auch stabilsten Dachmaterialien überhaupt. Mit nur vier Dachplatten kann ein ganzer Quadratmeter Dachfläche eingedeckt werden. 8 PREFA Farben und ein umfangreiches Zubehörprogramm sorgen für optisch anspruchsvolle und extrem langlebige Dächer. Das PREFA Langzeitdach, Mittelpunkt eines perfekt aufeinander abgestimmten Komplettprogramms rund ums Dach, ist das Ergebnis permanenter Forschungsarbeit und härtester Praxistests des führenden, österreichischen Aluminium-Dachspezialisten PREFA. Grundmaterial für die PREFA Aluminiumprodukte sind Legierungen nach EN 1396. Die Beschichtung der Dachplatten, Dachschindeln, Dachrauten, Dachrinnen, Rohre und Bleche erfolgt im Coil-Coating-Verfahren und unterliegt den strengen Auflagen der ECCA (European Coil Coating Association) in Brüssel. 40 Jahre Garantie auf das Aluminiumgrundmaterial der PREFA Dachplatten, PREFA Dachschindeln und PREFA Dachplatten gegen Bruch, Rost und Auffrieren bei natürlicher Umweltbelastung und fachgerechter Verlegung durch den Bauspengler!" (IFCLABEL)
  ePset_ManufacturerProductInformation | properties | on 3 objects (3 IFCWALL)
    Category = "https://ch.buildup.group/category/91c1ed6a-ab21-4a53-a8d8-be9a0c06753e/view" (IFCLABEL)
    Description = "" (IFCLABEL)
  ePset_ManufacturerProductInformation | properties | on 2 objects (2 IFCSTAIR)
    Category = "https://ch.buildup.group/category/a4d9a09a-f7f0-4da2-959a-6aa482156caa/view" (IFCLABEL)
  L10.2 | properties | on 24 objects (21 IFCWALL, 3 IFCSLAB)
  L10.1 | properties | on 1 object (1 IFCSLAB)